1. Modify boot.S, so that your kernel switches to EL0 (instead of switching to EL1).

[please upload a separate tar ball]

1. After landing in EL0, can your kernel print out the current exception level? If so, how? If not, why?
2. Describe in a short paragraph: what will happen if we execute an eret instruction at EL0?